# KS83301A/KS83301B *Bluetooth*® Low Energy 4.2 Signaling, KS83302A/KS83302B WLAN b/g/n Signaling,

# KS83304B *Bluetooth*® Low Energy 5.0 Signaling and Zigbee 3.0 signaling Measurement Suites

## Version 2019.1113

* The driver now supports both 34999A (requires firmware 15.07) and 34999B modules (requires firmware 20.02). File name is changed to Keysight.34999.dll to reflect this change.
  + KS83301B/A can only run on the 34999A module.
  + KS83302B/A can run on both 34999A and 34999B modules.
  + KS83304B and KS83305B can only run on the 34999B module.
  + Renamed 34999A in Bench Settings to 34999.
* Enhance the operation of active scan PER measurement and PER power sweep.
* Raw results of advertising Intervals are now included into the report.
* Added timestamp in simple csv listener.
* Added log information of the source of scan interval used in active scan related step.

Issue resolved:

Connection for PER measurement