{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,0,3,3]]}
["Keysight EDU36311A diode curve example program. Compatible with Keysight IO library suite 2021  www.keysight.com/find/iosuite",null,null,null,null,"Visa address:","USB0::0x2A8D::0x8F01::CN60460025::0::INSTR"]
[null,null,null,null,null,"Steps:",11]
[null,null,null,null,null,"Curr limit:",0.7]
[]
[]
[]
["Voltage VD (V)","ID (A)"]
[0.2,9.114002E-5]
[0.4,1.016932E-4]
[0.6,2.8748580000000001E-3]
[0.65,8.7653990000000001E-3]
[0.67500000000000004,1.4710640000000001E-2]
[0.7,2.586254E-2]
[0.72499999999999998,4.6057420000000002E-2]
[0.75,8.3259070000000004E-2]
[0.77500000000000002,0.1540416]
[0.8,0.2651772]
[0.85,0.70187489999999997]