**U1115A Firmware Update Procedure**

1. On the U1115A, change the “Role” to “Slave” by following the steps below.
	1. Connect 🡪 Bluetooth 🡪Edit 🡪  🡪 OK
2. Right click on the PC Bluetooth icon.
	1. Click on “Add a Device”.



* 1. Select the U1115A to be connected and click on “Next” to proceed.

Note: different U1115A units will have different MAC address.



* 1. Click on “Enter the device’s pairing code”.



* 1. Key in pairing code “1234” and click “Next” to proceed.



* 1. The message below will appear when the pairing is successful.



1. Right click on the PC Bluetooth icon.
	1. Click on “Show Bluetooth Devices”.



* 1. Right click on the U1115A unit connected 🡪 Properties



* 1. Click on the “Hardware” tab to see the COM port which the U1115A unit is connected to.

Note: Different PC might have different COM port value.



1. Double click on “U1115AFirmwareUpdatePackage”.



* 1. Select the COM port as per Step 3(c).

Note: if the COM port value does not appear in the drop down list, please click on “Update Port” to refresh the COM port list.

 

* 1. Click “Connect” and wait until the “Start” button is enabled.

 

* 1. Click on “Start” and wait until the programming is complete.



1. You may check the firmware version by following the steps below.
	1. Settings 🡪 More 🡪 System 🡪 Sys Info

 

After programming

1. Set the unit to factory default setting by following the step below.
	1. Settings 🡪 More 🡪 System 🡪 Reset 🡪 Yes

Unit will reboot automatically.